;=====================================================
;
;   S190WL.inf         Ver. 1.0      04/26/2011
;
;   Copyright (C) 1999-2009 Acer Inc.
;
;   This is a Microsoft Windows setup information
;   file for the Acer Color Monitor.
;
;=====================================================
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%Acer%
DriverVer=04/26/2011, 1.0.0.0

; Ensure to add directive below with the proper catalog file after WHQL
; certification
CatalogFile=S190WL.cat

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
DefaultDestDir=11
S190WL_Analog.copyfiles = 23
S190WL_Digital.copyfiles = 23

[SourceDisksNames]
1=%SourceDisksNames%

; Enable the following section to copy a monitor profile
[SourceDisksFiles]
S190WL.icm=1

[Manufacturer]
%Acer%=Acer,NTx86,NTamd64

[Acer]
%S190WL_Analog%=S190WL_Analog.Install, MONITOR\ACR02A0
%S190WL_Digital%=S190WL_Digital.Install, MONITOR\ACR02A0

; Modify the hardware ID (ACR02A0) to match that of the monitor being used
[Acer.NTx86]
%S190WL_Analog%=S190WL_Analog.Install, MONITOR\ACR02A0
%S190WL_Digital%=S190WL_Digital.Install, MONITOR\ACR02A0

; Modify the hardware ID (ACR02A0) to match that of the monitor being used
[Acer.NTAMD64]
%S190WL_Analog%=S190WL_Analog.Install, MONITOR\ACR02A0
%S190WL_Digital%=S190WL_Digital.Install, MONITOR\ACR02A0

[ControlFlags]
ExcludeFromSelect.NT=Monitor\ACR02A0
ExcludeFromSelect.NT=Monitor\ACR02A0

[S190WL_Analog.Install]
ACRReg=ACR_CURRENT_REG
AddReg=S190WL_Analog.AddReg, 1440, DPMS
CopyFiles=S190WL_Analog.CopyFiles

[S190WL_Digital.Install]
ACRReg=ACR_CURRENT_REG
AddReg=S190WL_Digital.AddReg, 1440, DPMS
CopyFiles=S190WL_Digital.CopyFiles


[ACR_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

; Pre-defined AddReg sections. These can be used for default settings on
; a given standard resolution is used.

[1440]
HKR,,MaxResolution,,"1440,900"

[DPMS]
HKR,,DPMS,,1

[S190WL_Analog.AddReg]
HKR,"MODES\1440,900",Mode1,,"31.0-80.0,56.0-76.0,-,+"
HKR,,ICMProfile,0,"S190WL.icm"

; Enable the following section to copy a monitor profile
[S190WL_Analog.CopyFiles]
S190WL.ICM


[S190WL_Digital.AddReg]
HKR,"MODES\1440,900",Mode1,,"31.0-80.0,56.0-76.0,-,+"
HKR,,ICMProfile,0,"S190WL.icm"

; Enable the following section to copy a monitor profile
[S190WL_Digital.CopyFiles]
S190WL.ICM

[Strings]
MonitorClassName="Monitor"
Acer="Acer Inc."
SourceDisksNames="Acer Inc. Monitor S190WL Installation Disk"

S190WL_Analog="S190WL(Analog)"
S190WL_Digital="S190WL(Digital)"


