**
**
**  VIA Networking Velocity Family Gigabit Ethernet Adapter
**
**  NDIS Driver for Windows Vista X64
**
**  v1.45   May 2012
**
**

Introduction:
=============

  This document shows you how to setup the driver in Windows operating system.


Contents of the Subdirectory:
=============================
    
    GET6X64V.SYS        The NDIS6 driver for Windows Longhorn.
    GETNDX64.INF        The installation information file.
    DIFxAPI.DLL         DIFx API for Vista X64.    
    VUINS64.DLL         64-bit uninstaller.
    WIN64.TXT           This file.


Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Turn on the power of your PC on to boot from Windows operating system.
       Windows will auto-detect your new adapter, and the "New Hardware Found"
       dialogue box will appear. Select "Driver from disk provided by hardware
       manufacturer" to install driver from the diskette that comes with your
       LAN adapter.

    2. Insert the driver diskette into your floppy drive, and specify the
       path of the driver in the diskette(i.e. A:\) to copy the driver
       files to your system.
