Windows Vista x64 installation
-------------------------------

For Windows Vista x64, only the printer driver can be installed.
Note: If installing the B2540 as a network connection please follow the "How to Install the Companion Suite Pro LM TCP/IP Monitor Port" instructions below first.


1) Plug in the USB cable and switch on your device
2) When prompted for the "MF F@x" driver, choose "Don't show this message again for this device"
3) When prompted for the "XML interface" driver, choose "Don't show this message again for this device"
4) For the printer driver choose "Locate and install driver software".



Driver Only Install
-------------------

You can install the drivers, on their own, by using Plug and Play or Add Printer Wizard and browse to the root of this CD when prompted for the location of the driver.
Note: To install the driver as a network connection you must install and use “Companion Suite Pro LM TCP/IP Monitor Port”, this is listed as a “Local” connection.


How to Install the B2540 MFP Postscript Driver
-----------------------------------------------
To be able to install the Postscript driver you need to use the Adobe Universal PostScript Windows Driver Installer.

1) Visit www.adobe.com, and browse to the “downloads” section.
2) Search through the list of available downloads for "Printer drivers"
3) Click on “Update”, on the right hand side.
4) From the list of available options click on "Win"
5) From the list of available downloads choose "Adobe Universal PostScript Windows Driver Installer 1.0.6 - English"
	Note: At time of writing 1.0.6 was the current release
6) Proceed to download “winsteng.exe”
7) When the download is complete run the installer, by double-clicking the winsteng.exe.
8) Follow the onscreen instructions, until “Select a Printer Model” screen appears.
9) From the “Select a Printer Model” screen, select “Browse” and browse to “D:\Driver\PPD\English” (Where D: is the CD-Rom).
10) Choose “Oki B2540(PS)” and click “Ok”.
11) Click “Next” and continue with the onscreen instructions. 

Once the installer has finished the driver will be ready to use.

Note: To install the driver as a network connection you must install and use “Companion Suite Pro LM TCP/IP Monitor Port”, this is then listed as a “Local” connection.


How to Install the Companion Suite Pro LM TCP/IP Monitor Port
------------------------------------------------------------- 
To use the B2540 MFP as network printer you must use the Companion Suite Pro LM TCP/IP Monitor Port.

1)	Open the “Printers folder”.
2)	Choose “File->Server Properties”
3)	On the displayed dialog choose the “Ports” tab.
4)	Click on “Add Port..”
5)	Click on “New Port Type”
6)	Browse to “D:\” and click “Open” (Where D: is the CD-Rom)
7)	Click “Ok”, this will start the install of the Monitor Port
8)	From the List displayed choose “Companion Suite Pro LM TCP/IP Monitor”, and click “New Port”
9)	Enter the details for the new port
10)	Click “Ok”, and during the printer install this port will be available.

