Synaptics Driver Release Notes for HPConsumer
OS: 32-bit and 64-bit Windows 7, Windows 8, Windows 8.1 and Windows 10
Languages Supported: English, Arabic, Portuguese (Brazil), Croatian, Czech, Danish, French, French Canadian, Finnish, Greek, German, Hungarian, Indonesian, Hebrew, Italian, Japanese, Korean, Spanish (Mexico), Dutch, Norwegian Bokmal, Polish, Portuguese, Romanian, Russian, Swedish, Slovakian, Spanish (Spain), Slovenian, Thai, Turkish, Traditional Chinese, and Simplified Chinese.
Version: 19.3.11.31 Date: 06-21-2016

Issue Number | Description | Root Cause | Solution
--- | --- | --- | ---
HDR-33586 ✓ | [HPConsumer, Win10] Multiple Finger Tapping incorrectly reported. | We have some feature improvment since v19.3.10 and it seems not cover some cases for tapping count change. | Temporarily revert back to previous code.

Version: 19.3.11 Date: 06-02-2016

Issue Number | Description | Root Cause | Solution
--- | --- | --- | ---
HDR-33415 ✓ | pointing function was intermittent after boot into OS then use TP | The EC keep sending multiple scan code during boot into OS. This caused the touchpad to be suppressed when we got hotkey. The ignore scan code settings for "E057" in inf was already there. However, there are some implementation changes in latest driver where we miss to get parameter of ignore scan code settings. | Retrieve parameter settings for ignore scan code.

Version: 19.3.10 Date: 05-27-2016

Issue Number | Description | Root Cause | Solution
--- | --- | --- | ---
HDR-33314 ✓ | [Win10 HPConsumer] 1F and 2F Horizontal Scroll becomes Vertical Scroll in MS Photos | Scrolling settings specifically within MS Photos was not enabled for this platform. | Turn on Scrolling settings for MS Photos for this platform.
HDR-33340 ✓ | HP ‘s request: please hide Synaptics Pointing Device from notification in PNPID SYN3241 | Customer request to hide the tray icon notification for SYN3241. | Hide the tray icon of ClickPad for SYN3241.

Version: 19.3.9 Date: 05-20-2016

Issue Number | Description | Root Cause | Solution
--- | --- | --- | ---
HDR-33229 ↻ | Change Palm Rejection Behavior on Miniport PTP |  |
HDR-33307 ✓ | HP_UXUI - v19.3.8 - Windows photo viewer does not support the rotate function | When we enable rotation feature for Microsoft Photos in win8.1 (it is a Metro app in win8.1), rotation settings for win8.1 (use Ctrl + .) accidentally overrides settings for win10 (Ctrl + R) that was set as default in previous versions. | Besides default and settings for win8.1, add Rotation settings for Microsoft Photos in win10 specifically.
HDR-33314 ✓ | [Win10 HPConsumer] 1F and 2F Horizontal Scroll becomes Vertical Scroll in MS Photos | Scrolling settings specifically within MS Photos was not enabled for this platform. | Turn on Scrolling settings for MS Photos for this platform.
HDR-33327 ✓ | 19.3.8 HPConsumer WHLK failed with BSOD issue. | SynRMIHID driver tried to copy memory with incorrect data length during Win10 HLK test. | The driver should check the memory size and don't copy memory if it is invalid. This addressed the WIn10 HLK BSOD issue.
HDR-33228 ✓ | 4F Flick to Switch Virtual Desktop Since Windows 10 Build 14328 |  | Added code to support 4F Horizontal Flick gestures to switch virtual desktops. This is a new Windows 10 touchpad feature.

Version: 19.3.8 Date: 05-18-2016

Issue Number | Description | Root Cause | Solution
--- | --- | --- | ---
HDR-33228 ✓ | 4F Flick to Switch Virtual Desktop Since Windows 10 Build 14328 |  | Added code to support 4F Horizontal Flick gestures to switch virtual desktops. This is a new Windows 10 touchpad feature.

Version: 19.3.7 Date: 05-06-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32331 | Implement the new control flow work with FW new lid behavior. | implement PS/2 set sleep mode feature.
HDR-32973 | HP request when TP disable, "defaults" should be gray out | Disable the default settings button when touchpad device is disabled.

Version: 19.3.6 Date: 04-29-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-33011 | PNPID request: SYN3245, SYN3246, SYN3247, SYN3248 | Add PNPID SYN3245, SYN3246, SYN3247 and SYN3248
HDR-33012 | PNPID request: SYN3249, SYN324A | Add PNPID SYN3249 and SYN324A
HDR-33097 | PNPID request: SYN324B the same setting as SYN3224 | Add PNPID SYN324B

Version: 19.3.5 Date: 04-22-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32896 | Remove button action process from enabling/disabling device | Merge from branch: remove button action process from disabling/enabling TP
PRJ-35772 | Add bootloader v7 and v8 Support in SynReflash | Fixed block size in bootloader V5/6

Version: 19.3.4 Date: 04-15-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32107 | Create PTP injection code to replace touch injection | Add code to support PTP injection in kernel

Version: 19.3.3 Date: 04-08-2016

Issue Number | Description | Fix Comment
--- | --- | ---
SWT-459 | EFU shall support installation with silent mode | SynReflash Configuration shall support installation with silent mode
HDR-32703 (1270567) | SIO1270567 - SFT-TP-IEC/Circus:Two finger Rotate have no function by Foxit PDF Reader. | Add rotate for Foxit and Nitro PDF Reader.; Fix a copy/paste error; Add horizontal scrolling for Foxit and Nitro PDF Reader.

Version: 19.3.2 Date: 04-01-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28669 | [Linux_Ubuntu 14.04] "Two Button Click Action" description should display in Buttons settings. | using consistent item code for 'text', 'combo list' and 'configure'.; [linux] Merge linux section into hpnewui for the trunk.
HDR-32107 | Create PTP injection code to replace touch injection | Add code to support PTP injection in kernel
HDR-32624 | Add 3+2BCP PnPIDs in Linux driver | [linux] build correct section for x86 or x64.
HDR-32734 | There is no pop-up message when connecting an external USB mouse | Better way: dont initialize the value on child class. Balloon not working on seperated TP and CB trayaction.
PRJ-35772 | Add bootloader v7 and v8 Support in SynReflash | Add bootloader v8 and UPP Support in SynReflash
HDR-32216 | Please set PNPID SYN323D as convertible platform | Modified settings for SYN323D
HDR-32598 | ZOOM in/out too smooth issue | Adjust pinch scale for HP Panini 1.0
HDR-32776 | PNPID request: SYN3244, HPConsumer | Add PnPID SYN3243 and SYN3244 for HPConsumer.inf

Version: 19.3.0 Date: 03-18-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32331 | Implement the new control flow work with FW new lid behavior. | implement PS/2 set sleep mode feature.; Found a logic error....; Fix an issue that SMBus device won't correctly call RMI's WriteDeviceSleepMode
PRJ-35774 | Driver Upgrade Issues | Changed code to fix SMBus driver upgrade incompatibily issue. Take out OEM DelReg
HDR-32216 | Please set PNPID SYN323D as convertible platform | Modified settings for SYN323D
HDR-32655 | PNPID request: SYN3242, inf: HPConsumer | New PNPid SYN3242.

Version: 19.2.17 Date: 03-11-2016
System enhancements
Version: 19.2.16 Date: 03-03-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31582 | [Win10, HPConsumer Gummi] Incorrect type of ClickPad shown in Video | Fixed incorrect type of ClickPad in video. There is no control zone platform for HP.
HDR-32504 | PNPID request: SYN3240 SYN3241 | PNPID request: SYN3240 SYN3241
HDR-32525 | default setting of Advanced filter is wrong in v19.2.11.34_HPConsumer group132 | Config for Advanced filter size.

Version: 19.2.15 Date: 02-25-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32442 | SMBus driver support for new AMD CPU Stoney | SMBus driver support for AMD Stoney.
HDR-32462 | PNPID request: SYN323F, inf: HPConsumer | Add PNPID SYN323F

Version: 19.2.14 Date: 02-18-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31904 | HP request to enable pinch/zoom when both 2 finger are moving | Enable pinch to zoom when two fingers moving in different direction

Version: 19.2.13 Date: 02-12-2016
System enhancements
Version: 19.2.12 Date: 02-05-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32202 | Sometimes TouchPad Button doesn't work on login screen | We should update Button Status when lid close/open disable device is called. The function EnableButtonActions called in DisableDeviceAndButton will check the setting "ButtonsEnabledDisabledWithDevice" So it won't break the feature that button disable/enable which should be independent from touchpad device disable/enable state.
HDR-32319 | [HID/USB] Observed opposite scroll direction while performing 2F edge motion scroll in MS Edge | Fix injection bug (reverse scroll doesn't work)
HDR-31951 | 1F and 2F Horizontal Scroll fail to work in powerpoint | Applied touch injection for scrolling on MS PowerPoint
HDR-32125 (SIO1253795) | "Default Settings" show cut off on ABE(SP) image with FHD units | Fixed string cut off in Spanish
HDR-32255 | please help check group149, customer report "Touch sensitivity slider" show 1.5/6, it should be 2/6 | Changed sensitivity slider min, max and frequency to meet default value change in the driver
HDR-32283 | please set PNPIDSYN323B, SYN323C, SYN323E as convertible platform, the same as SYN321B | Modify settings for SYN323B, SYN323C and SYN323E

Version: 19.2.11 Date: 01-28-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31803 | HP report a SmartSense bug | Porting to trunk. Modified the palm check filter to update timeout start stamp when finger in edge zone.
HDR-32159 | SIO1257515 - SFT_Touch_HOU/Riata/SI : Jumpy cursor movement observed | Don't decode normal double tap if it is decoded for other actions, this avoids double actions for one double tap.
HDR-32215 | PNPID request: SYN323E for HPConsumer | Add PNPID SYN323E

Version: 19.2.10 Date: 01-21-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32076 | please modify back keyboard stroke time of pike | Roll back the setting for keystroke time
HDR-32078 | [HPConsumer RMIHID]Clicking Palm still occurs in HP Split x2 system | Fixed clicking palm for HP Split x2
HDR-32104 | [Win10, HPConsumer, Saffron] Startoing zone disappears | Add starting zone settings
HDR-32119 | [HPConsumer] Add PNPIDs SYN323A to SYN323D | Add PNPIDs SYN323A to SYN323D

Version: 19.2.9 Date: 01-14-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31756 | Cursor suppressed from moving sometimes when moving the cursor on the desktop for mini port driver | Add PalmCheck thresholds for PTP miniport driver withACM2.1
HDR-31649 | please help remove the version information in control panel "Synaptics ClickPad" | Apply the device name format to all PNPIDs
HDR-32060 | please add ApolloLake SMBus HWID into driver | Support new SMBus controller of Intel ApolloLake.

Version: 19.2.8 Date: 01-07-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31942 | Tray icon lost but SYNTPENH still exsit | When someone had deleted our tray icon, the error code should be ERROR_TIMEOUT. Shell_NotifyIcon can't be deleted or modified before we add new tray icon. We should check correct error code and add tray icon again.; Restart SynTPEnh while tray icon can't refresh
HDR-30535 | [HPConsumer] Clicking palm occurs | Fixed palm clicking
HDR-31649 | please help remove the version information in control panel "Synaptics ClickPad" | Removed the version of device discovery enhancement entries in Windows control panel
HDR-31822 | HP Saffron: keyboard cann't enter into OS when resume from S3/S4(enter into S3/S4 from login interface) | Fixed enter key cannot unlock the lock screen when resume from S3/S4
HDR-31931 | please set PNPID SYN322D 322E 322F and 3237 as the same as SYN3220 | Modified group settings
HDR-31940 | please set PNPID SYN3238 and SYN3239 the same as SYN3228 | Set PNPID SYN3238/SYN3239 to be the same settings as SYN3228
HDR-31970 | Quanta report Rotate should be "checked" in PNPID SYN3225, SYN3226, SYN322B, SYN322C | Enable rotating on Win10 for PNPIDs

Version: 19.2.7 Date: 12-17-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31450 | 3F drags and slides video | Fix win10 3 finger vertical slide video
HDR-31882 | Change finger threshold to match FW for Imaging Sensor TP | Changed slider min, max and frequency to meet defautl value change in the driver.; Changed finger threshold to match FW for Imaging Sensor TP

Version: 19.2.6 Date: 12-11-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31430 | 2F scrolling will cross more than one page on "photos” and "IE” | Injection for scrolling gesture in Microsoft Photos app should start from app window center rather than from the cursor.
HDR-31820 | please set PNPID SYN322B and SYN322C as the same group as SYN3225 and SYN3226 | set SYN322B/SYN322C to be the same group as SYN3225/SYN3226.

Version: 19.2.5 Date: 12-03-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31713 (109532) | Synaptics TP has no Scrolling function by Windows Photo Browser | Send only 1 finger position for metro photos
HDR-31743 | Report rate calculation is wrong on non-PS2 platform if there are more than 1 finger on the pad | Fixed a wrong logic that causes the driver uses wrong report rate for MF case.
HDR-31756 | Cursor suppressed from moving sometimes when moving the cursor on the desktop for mini port driver | Don't convert non-finger to palm for miniport driver.
HDR-31653 | ForcePad: Separate the threshold for checking suspicious force | The default value has been set to efrfCheckForce in constructor
HDR-31738 | please add solution of HDR-29577 into below new PNPID | Porting the fixes for HP Candy to trunk

Version: 19.2.4 Date: 11-26-2015
System enhancements
Version: 19.2.3 Date: 11-19-2015

Issue Number | Description | Fix Comment
--- | --- | ---
PRJ-35733 | Inertia, coasting and edge motion support for TouchInjection | Make scroll speed adjustment supported in touch injection
HDR-31653 | ForcePad: Separate the theshold for checking suspicious force | Separate the theshold for checking suspicious force
HDR-31664 | Update Exit code in setup installation for non Dell inf | Update Exit code for Installation log

Version: 19.2.2 Date: 11-12-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31551 | Add PS2 query $11 | Added PS2 $11 query for integrated stick
PRJ-35733 | Inertia, coasting and edge motion support for TouchInjection | Add 1 finger chiral scroll supported in touch action. add some performance fix
HDR-31544 | PNPID request: SYN322B to SYN3239, inf: HPConsumer | Add PnPID SYN322B to SYN3239
HDR-31561 | Review the TouchBuffer mechanism | Review the TouchBuffer mechanism
HDR-31581 | PNPID request: SYN323A, SYN323B, inf: HPConsumer | Add PNPID SYN323A and SYN323B

Version: 19.2.1 Date: 11-06-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-12003 | Review location of driver parameters | Moved some registry from HKLM\system.... to HKLM\Software\Synaptice\.. because they are put in wrong place.; Fixed a build error.
HDR-12577 | remove the m_pPluginAction from the zone | Removed the m_pPluginAction from the zone.
HDR-28430 | The "Help" Window of Edge Swipes function show blank. | Added help for edge swipe in sgsnewui..

Version: 19.2.0 Date: 10-29-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31431 | Touchinjection error occurs when lifting one finger up during 2 finger gestures | Fix injection error. If the lifted up finger is finger 0 then we have no chance to go into slide to call cancel action of touch action, and we also do not contine to feed in moving finger of touch screen, then OS will found we time out to feed in touch screen packet and neither to send a finger up packet to end the stroke, then there is time out error.
PRJ-35733 | Inertia, coasting and edge motion support for TouchInjection | Add code to make touch injection support 1 finger scrolling. And fix a bug
HDR-30535 | [HPConsumer] Clicking palm occurs | Fixed clicking palm
HDR-31388 | Many PnPIDs in HPConsumer.inf can't be installed. | some sections in INF are wrong or missed which leads to installation failure for Syn1EAD, SYN3214~SYN3216, SYN3225~SYN322A.

Version: 19.1.3 Date: 10-22-2015

Issue Number | Description | Fix Comment
--- | --- | ---
|  | New language translations for Windows installer, help files and control panel
HDR-31326 (ECR358436) | Vertical/Horizontal Swipe checkbox under three fingers will auto be checked when switch tab in Gesture. | The hidden control should not get or set settings
HDR-31349 | Add back the logs for KTL Enhancement | Adding back KTL Enhancement log for different Stroke State.
|  | We still need to install SMBus driver for FW with SMBus bootloader.
HDR-31309 | PNPID request: SYN321E SYN321F SYN3220, HPConsumer | Add PnPID SYN321E, SYN321F, SYN3220 in HPConsumer.inf
HDR-31310 | PNPID request: SYN3221, SYN3222, SYN3223, SYN3224, HPConsumer | Add PNPID SYN3221, SYN3222, SYN3223 and SYN3224
HDR-31328 | PNPID request: SYN3225; SYN3226, HPConsumer | Add PnPID SYN3225, SYN3226 in HPConsumer.inf
HDR-31355 | PNPID request: SYN3227 SYN3228 SYN3229 SYN322A | Add PnPID SYN3227, SYN3228, SYN3229, SYN322A in HPConsumer.inf

Version: 19.1.2 Date: 10-15-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31282 | Add log for lid switch callback event | Add log event for lid switch
HDR-31287 (1222833) | SIO1222833 - FNC_PE_COMPAL/Aria/ Win8.1: Cannot switch pictures to the previous or next in MS photos when using three fingers flick to left or right | fix an issue that 3F-flicking failed for MS Photos in win8.1

Version: 19.1.1 Date: 10-08-2015
System enhancements
Version: 19.0.27 Date: 09-29-2015
System enhancements
Version: 19.0.26 Date: 09-29-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30955 | Win 10 PTP like 3 finger gesture: We should do nothing when doing 3 finger horizontal flick in task switcher window with "new desktop" button | Fix win10-like 3 finger flick issue in new windows internet browser. And add emit; Change win 10 PTP like 3 finger flick gesture behavior
HDR-31037 | When connect 2 PCs using a usb file transfer cable, and then use the mosue to move cursor between 2 PCs, then do 3 finger flick down, the behavior is not correct | fix win 10 like 3 finger flick issue
HDR-30778 | PNPID request: SYN3218 SYN3219 | disable rotate for win10
HDR-31007 (1215031) | SIO1215031 - FNC_PE_HOU/Ceasars/SI3 :Win 10 is not included in Synaptics release notes. | Add Windows 10 to list of supported OSes in the release notes
HDR-31013 | please remove 3F and 4F tap in below PNPID | Hide 3F and 4F tapping
HDR-31027 (1215969) | SIO1215969 - M-SHA-FIT/Sands: 'Show Tray Icon in Taskbar' in Mouser Properties will be greyed out when disable touchpad | Don't grey out "Show Tray Icon in Taskbar" control if the TP is disabled.

Version: 19.0.25 Date: 09-10-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30773 | [ Win10] Alt + Tab / 3 finger left - right swipes to switch application function can be triggered after put 1 finger on the touchpad then do zoom / pinch gesture by another 2 fingers. | If one finger is not in resting zone, the other 2 fingers perform pinch gesture, then when thease 2 fingers lift up, we might triggered the 3 finger flick gesture. We should always do the finger direction check no metter the finger counts
HDR-30887 | Press Win + M to minimize all windows then Press Win + Tab to launch task switcher, then do 3 finger flick it will close the task switcher | Fix win10-like 3 finger flick up bug
HDR-30922 | Double tap to disable the touchpad it shows "ON" at the Mouse & touchpad | Wrong logic, a TP enable/diswable hot key only was sent to disable TP, otherwise the TP is disabled, there is no chance to sent the hotkey to enable it.
HDR-30864 | HP Gummi: Please change he setup information file of the Syna driver to support TLC2 instead of TLC4 | Updated top level collection of HP Gummi
HDR-30886 | HP Gummi: Click will be trigged by palm | Enabled ClickSmart

Version: 19.0.24 Date: 09-04-2015

Issue Number | Description | Fix Comment
--- | --- | ---
PRJ-35570 | Change coinstaller and setup program to install HID/SMB miniport driver | Added Dpinst exit code
HDR-28105 | 2F EdgeMotion Scroll does not work in Win Reader | TouchInjection cannnot support 2F EdgeMotion and Inertia (Coasting). For the reported Win Reader and MS Edge app, we need use our generic scrolling algorithms.
HDR-30778 | PNPID request: SYN3218 SYN3219 | add PNPID SYN3218/SYN3219
HDR-30804 | HP Gummi: right button area should be 30% in X-axis | Adjust button zone size

Version: 19.0.23 Date: 08-27-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30012 | [Win10] Synaptics Startup Program in Windows 10 in comparison with Windows 8.1 | Remove run key if we use service to launch enhancement for all windows; Remove run key to start up SynLenovoHelper.
HDR-30634 | PNPID request: SYN3217 in HPConsumer and HPConsumer_HIDmini | Add PNPID SYN3217; Add PNPID SYN3217
HDR-30739 | [HPConsumer] Coasting does not work when PDF file opened in Microsoft Edge | TouchInjection cannot support the costing featues. Disable TouchInjection on Microsoft Edge to enable the coasting feaures on SMB group 129.

Version: 19.0.22 Date: 08-20-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30524 | [HPConsumer] Alt+B shortcut key duplicates and does not work in Mouse Property Window | Updated shortcut keys for duplicates
HDR-30532 | [HPConsumer] Clickpad is not disabled after resuming from S3 in slate mode | Fixed TouchPad has function after resume from S3 on slate mode

Version: 19.0.21 Date: 08-13-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30303 | Please add localized help message for Windows 10 3F and 4F gestures | Fix "Maximum" and "Minimum" translations in Windows 10 gestures
HDR-30339 | Fail to uninstall driver from Win10 Settings: Apps & Features | Add detailed driver unstallation to the log log; Get original install dir of synpd oem inf to the log
HDR-30474 | Button comb box is not greyed out in PTP mode | Greyed out buttons combbox when the TP is switched to PTP.
HDR-30221 | In UI help of "Two-finger Tapping", the description is for "Two-finger click" | Fixed Help string of two-finger tap
HDR-30503 | please set Tray Icon is "Remove tray icon from taskbar" in below PNPID | Remove tray icon from taskbar for PNPIDs

Version: 19.0.20 Date: 08-06-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30458 | Turn off ALT+SHIFT+L to dump log file by default | Turned off using "ALT+SHIFT+L" to collect a log file because it affect some apps which use these hot key.
HDR-30397 | please change PNPID:SYN3214 to PS2 interface | Change SYN3214 to PS2 interface
HDR-30442 | HP Rocher: Rotate doesn't work on Win10 photos | Fixed rotating doesn't work on Win10 photos
HDR-30443 | HP Rocher: Error message will be pop up when click "tapping" item 1st time | Fixed error message of html

Version: 19.0.19 Date: 07-30-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30170 | Marking resources as non-discardable | Marking resources as non-discardable
HDR-30268 (1197171) | 1197171 - FNC_PE_ /Aria & Venetian: In the drop down box of Button Action (Button /Zone completely disabled) repeat on Touchpad (TouchStyk) tab | Fixed plugin action list item repeat issue when there is only one plugin action; Removed all plugin actions for LRM buttons.
HDR-30339 | Fail to uninstall driver from Win10 Settings: Apps & Features | Add unstallation log ton Synaptics.PD.log; Hide command prompt windows in installation; Hide command prompt windows which remove SynTPEnhService in uninstallation; Add last step in finish install lon Synaptics.PD.log; Fixed cannot uninstallation driver from Win10 - Settings - Apps & features

Version: 19.0.18 Date: 07-23-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30262 | Use major version for HID/I2C in miniport driver | Changed FW version report format in miniport HID descriptor, for HID/I2C platform only major version is used, for InterToutch the version formation is major(8-bit).minor(8-bit).
HDR-30270 | Set ShareVector to TRUE which allows IRQ sharing in SMB | Set ShareVector to TRUE which allows other devices sharing interrupt with SMB.
HDR-30271 | Report max finger report count the same as FW in HID so we can support reported fingers less than 5 | Reported max finger report what FW reports instead of hard coded 5 in miniport driver HID descriptor so we can support less than 5 fingers.
HDR-30138 | PNPID request: 320F, 3210, 3211, 3212, and 3213 in HPConsumer | Correct the ID from 320E to 320F
HDR-30152 (1192472) | 1192472 - FNC_PE_Quanta/RRRR/win7:The tp driver version in "regedit" and "Synaptics.txt" show inconformity. | Create log when install driver not by setup.exe
HDR-30203 | IEC report 3finger tap and 4finger tap are shown in Win7 | Only enable the UI controls of three finger and four finger tapping on Win10
HDR-30208 | • When button is clicked, can activate pinch/zoom gesture with 2nd finger. Please refer to attached logfile. | Fix pinch to zoom could work when button clicked
HDR-30209 | PNPID request: SYN3214, 3215, 3216 in HPConsumer | Added settings for PNPID SYN3214, SYN3215 and SYN3216

Version: 19.0.17 Date: 07-17-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-30055 | Improve SMB data read performance | Combined F01 read with partial F11 and skipped F11 relative and gesture data for SMB so we can reduce SMB bus traffic.
HDR-30149 | Un-installation is not clean at the registry and C:\Program Files | Prevent restart too early in uninstallation
HDR-30171 | Report real FW version through miniport driver instead of hard coded 0 | Reported real FW version through miniport driver to OS for miniport driver PTP.
HDR-30138 | PNPID request: 320F, 3210, 3211, 3212, and 3213 in HPConsumer | Add id 320F/3210/3211/3212; modify id 320F/3210/3211/3212/3213 disablegestures setting from Disable1FScrolling_4FFlick to Disable1FScrolling_Rotating_4FFlick in Win10
HDR-30152 (1192472) | 1192472 - FNC_PE_Quanta/RRRR/win7:The tp driver version in "regedit" and "Synaptics.txt" show inconformity. | CoInstaller need to clean old install log file Synapitcs.log; Create log when install driver not by setup.exe

Version: 19.0.16 Date: 07-09-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29834 | Add a new control type | Add a new control type ToggleSwitch.
HDR-30055 | Improve SMB data read performance | Combined F01 read with partial F11 and skipped F11 relative and gesture data for SMB so we can reduce SMB bus traffic.
HDR-30081 | Dynamically create HID descriptor based on TouchPad type | Create HID descriptor based on TouchPad type either report 3 buttons or 1 button for miniport driver.
HDR-29785 | Video for Windows10 3F tap and 4F tap | Fixed video files for Win10
HDR-30008 | 3 finger flick is unchecked, please modify to checked | Enabled 3-finger flick
HDR-30009 | please set PNPID 1EFF and 1ED7 the same as 1EF0(group128) | please set PNPID 1EFF and 1ED7 the same as 1EF0(group128)

Version: 19.0.15 Date: 07-02-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29725 | Driver package to deprecate SynReflash tool from manifest | SynReflash will only be included in driver package if specified
HDR-29885 | Twist rotate is no function | Add Rotation support for Microsoft Window Photos App for win10
HDR-29964 | Branch Build Request v19.0.14.x ( _UltraNav_HidMini.inf) | Changed ACM confidence value to zero to allow using FW reported contact type and ignore confidence value if the slider is in the last slot.
HDR-29987 | Merge hpconsumer_rmihid to hpconsumer | Merged hpconsumer_rmihid to hpconsumer.

Version: 19.0.14 Date: 06-25-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28998 | Video for Windows 10 3F flick. | Added videos for Windows 10 3F gestures
HDR-29760 | please set PNPID setting of 1EDB, 1EC0, 1EC1 the same as 1EF0 | Modified default settings of PNPIDs
HDR-29809 | Driver setting modify: PNPID 1EFB, 1EFC, image sensor TouchPad | Driver setting modify in PNPID 3209 and 320A, profile sensor TP : PNPID 1EFB, 1EFC, image sensor TouchPad
HDR-29836 | Driver setting modify in PNPID 3209 and 320A, profile sensor TP | Driver setting modify in PNPID 3209 and 320A, profile sensor TP. Driver setting modify: PNPID 1EFB, 1EFC, image sensor TouchPad; Modified default settings for PS2 profile sensor touchpad.
HDR-29864 | please help add help string on Win10 | Modified the help strings of three finger flick and the naming of Two-Finger Tap; Modified the help strings of three finger flick on Win10; Modified the help strings of 3-Finger and 4-Finger tap on Win10
HDR-29896 | please set PNPID 1EC5, 1EC9, 1ECA the same as 1EF0(group128) | Driver setting modify in PNPID 3209 and 320A, profile sensor TP; please modify palmcheck-enhanced to SmartSense in PNPID 1EFB 1EFC; please set PNPID 1EC5, 1EC9, 1ECA the same as 1EF0(group128)
HDR-29897 | add two-Finger tap function in PNPID 3209 320A | Added two-finger tap for SYN3209 and SYN320A

Version: 19.0.13 Date: 06-18-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29759 | Please show FW version while query information in SynReflash | Fixed SynReflashPkg fail while image size over USHORT; Show FW version while query information under console
HDR-29573 | please add checked box for 3 finger tap and 4 finger tap, and set 3 finger click is middle button as default | Set three finger clicking action to middle button on Win10
HDR-29648 (1170293) | Zoom in/out is still available when only leave one finger to slide after perform two finger zoom in/out on TP | Cancel pinch action when finger count changed
HDR-29760 | please set PNPID setting of 1EDB and 1ECA the same as 1EF0 | 1. PNPID request: SYN320E in HPConsumer 2. set PNPID setting of 1EDB and 1ECA the same as 1EF0

Version: 19.0.12 Date: 06-11-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29609 | Missing ACM2 data when converting secondary finger packet to primary finger. | Moved ACM 2 data from secondary finger packet to primary finger packet when the packet is converted to raw packet.
HDR-29638 | BSOD when pressing any key | Fixed BSODs.
HDR-29671 | Remove sticky border control from all UIs | Removed sticky border feature from all control panel since this feature is rarely used by end users and also the driver cannot detect windows border correctly every time when there is a new OS release so we decided to remove this feature.
HDR-29425 | One finger horizontal slide would continue to execute Four-finger horizontal flick function after activated four-finger horizontal flick and click on clickpad surface | Fixed one finger slide could continue Flip3D function after the effect was triggered and should be cancelled by tapping or button clicking
HDR-29573 | please add checked box for 3 finger tap and 4 finger tap, and set 3 finger click is middle button as default | Fixed typo; Added three finger and four finger tapping on UI for Win10
HDR-29620 | please set PNPID 1ED1 the same as 1EF0 | Modified settings of PNPID 1ED1 to follow 1EF0
HDR-29689 | please set PNPID 1EB1 as PS2 interface | set PNPID 1EB1 as PS2 interface

Version: 19.0.11 Date: 06-04-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29039 | Video & Descrption for Windows 10 3F Swipe | New UI translations for Windows 10; New Windows 10 Translations for Enhancement
HDR-29188 (1154204) | 1154204 - FNC_PE_IEC/Bandit/W10:Error message pop out if Open control panel ->mouse when battery life is under 20% in DC mode. | Kept syntpenh run key in the registry even it is schedule by the scheduler because on Windows 10 if battery level is below 20%, the syntpenh is not scheduled.
HDR-29289 | touchpad takes 2 sec to enable after resume from s3, please check log file | Added ignore scan code
HDR-29467 (1153229) | 1153229 - FNC_PE_WIST/FFF/Win10:The LED on the touch pad turn amber when silent upgrade install. | Read non-configurable settings from registry only once insteadl of reading from APILoadState.
HDR-29573 | please add checked box for 3 finger tap and 4 finger tap, and set 3 finger click is middle button as default | Set three finger clicking action to middle button on Win10
HDR-29589 (1170283) | 1170283 - FNC_PE_Quanta/RRRR/Win10:The Search window(cortana)wouldn't popped up when use Three finger tap touchpad. | Rolled back to old method to decode the tap instead of new method for tap with more than 2F on PS2

Version: 19.0.10 Date: 05-28-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29283 | SynReflashPkg need to support more informations | Add packrat ID into file property while use SynReflashPkg to pack image and cfg
HDR-29353 | Change featurescore to 0xF9 per MS recommendation | Changed FeatureScore to 0xF9
HDR-28405 | Move HKLM to HKR in inf for WHCK Windows 10 compliant | Fixed SynTPEnhService failed to launch for non HiMini drivers when move HKLM to HKR; In driver update existing RunOnce key might disable SynTPEnhService for the new driver
HDR-29436 | PNPID request: SYN320C, SYN320D in HPConsumer | Added PNPIDs SYN320C and SYN320D

Version: 19.0.9 Date: 05-21-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29353 | Change featurescore to 0xF9 per MS recommendation | Changed FeatureScore to 0xF9
|  | Update DriverName to the one with UUID appends.
HDR-28405 | Move HKLM to HKR in inf for WHCK Windows 10 compliant | Fixed SynTPEnhService failed to launch for non HiMini drivers when move HKLM to HKR; Move HKLM to HKR
HDR-29030 | HPConsumer: please add Win10 gesture in HPConsumer | Added Win10 gesture and UI
HDR-29254 | PNPID request: SYN320B in HPConsumer | PNPID request: SYN320B in HPConsumer
HDR-29255 | In widnows application log, it will show many SynTPEnhService every 5 secs and then show resource insufficient | If syntpenh is launched prior than service, then the syntpenh launched by service should notify service not to launched again after it is gone.
HDR-29301 | BSOD 0xB8 on BJR SE | Processed reset interrupt in passive level instead of DPC level otherwise it will cause BSOD.

Version: 19.0.8 Date: 05-14-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-10618 | SynCOM samples have errors and warnings when compiling | mfctest; keypad; cPadClock; cPadImage; Disabler; Comtest; DisableGesture; SynDrumPad; BezelTest; SynWrapSample; SynPlot; SynDrumPad take out from SDK since it depends srd party library DirectX; SynView; SynForcePad; Dpn't include build bat files
HDR-13375 | Remove LAPACK copyright info | Copyright 2014 to 2015; Remove LAPACK copyright info
HDR-28137 | Un-installation driver is not clean | Use %ProgramFiles%\Synaptics\SynTP as temp dir to install auxiliary drivers instead of creating temp dirs in %ProgramData%
HDR-29104 | Change driver package name from SynARP | Update OS support information in SynPD.inf
HDR-26997 (FM: 2259) | This is a placeholder for build generated checkins. | Update ReleaseNotes.html
HDR-29011 | Apply Win10 gestures for HP Consumer | Enabled three finger flick on Win10
HDR-29107 | PNPID request: SYN3209 and SYN320A for HPConsumer | Added PNPIDs SYN3209 and SYN320A

Version: 19.0.7 Date: 05-08-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28137 | Un-installation driver is not clean | Un-installation driver is not clean - remove old SynTPCoInstaller; Use %ProgramFiles%\Synaptics\SynTP as temp dir to install auxiliary drivers instead of creating temp dirs in %ProgramData%; Always overwrite Coinstaller in update install
HDR-28874 | Incorrect ASIC Displayed in Diagnostics Window | Get correct ASIC type from F01 query 19.
HDR-29080 | Suppress Tap on Top Left Corner for SecurePad | Added code to suppress tap in the SecurePad notch area.; Checked whether query41 exists to find right offset for query43.
HDR-29102 | Update control panel to disable top left corner tap zone from UI | Hidden top left tap zone controls from the control panel.; Fixed a compiling error.
HDR-29103 | Update device type to SecurePad for SecurePad in the CPL to refer the device type | Updated device type to SecurePad in the CPL to refer the device type for SecurePad
HDR-29030 | HPConsumer: please add Win10 gesture in HPConsumer | Added Win10 gesture and UI
HDR-29064 | Add support for Neokylin Linux | Make sure libdbusc++ is linked in statically; [linux] linking dependencies.
HQA-10025 | Compal report Win7 WHCK Signed driver check fail | Put the aux driver files into drivers direcotry and prevent delete package file in destination dir in installation

Version: 19.0.6 Date: 04-30-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28622 | Tap zones can't work on the top right and top left corner | Allowed tap if a finger is in tap zone and object type is non-finger and tap zone is enabled.
HDR-28913 | Return code=-1 | Fixed return code for setup
HDR-29005 | [Win10, HPConsumer] Incorrect Mouse Properties Window shown after triggering Clickpad Setting from Tray Icon | Changed GUI code to fix mouse properties page wrong display issue.
HDR-29011 | Apply Win10 gestures for HP Consumer | Added Win10 gestures; Added Win10 gestures

Version: 19.0.5 Date: 04-23-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28907 | Correct Finger Packet State not for all fingers in a group but for those who are really in the zones | Correctly update Finger Packet State not for all fingers in a group but for those who are really in the left/right/resting zones
HDR-28944 (676644) | [Microsoft Windows 10 Team] [DeviceCompat][HID][CUET] : The check box setting "Disable internal pointing device..." in mouse properties under clickpad tab doesn't get applied. | Fixed checkbox out of sync issue when there are two tabs in the control panel such as Show tray icon in the taskbar or disable internal pointing device when external USB pointing device is attached.
HDR-28961 | The URL text of Win10 preview is cut off | Fixed URL text cut off on mouse properties page

Version: 19.0.4 Date: 04-16-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28877 | FNC_PE_HOU/Olympia 1.0/Synaptics I2C Mouse driver:Three-Finger Flick fails to work if undocking and docking tablet from base. | Reset OSD state variable when the device is removed or arriva otherwise currnet app will not be updated.l

Version: 19.0.3 Date: 04-09-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28774 | please help provide a registry to remove E0 57/E0 58 for LID open/close | Update scan code for LID open/close

Version: 19.0.2 Date: 04-02-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28731 | Add FeatureScore for all OEM INFs. | Fixed build errors.; Added FeatureScore in INF so OEM driver is always picked by WU first so the generic driver can be overridden in WU.
HDR-28736 | Change SMBus mode switch retry to zero | Removed SMBus mode switch retry from SwitchMode because there is a retry logic in the low level driver (retry 16 times).
HDR-28368 | please add HP 2015 consumer new feature into below PNPID | Ported to trunk. Added HP 2015 consumer new features

Version: 19.0.1 Date: 03-26-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28167 | Double click&Click lose function sometimes | Fixed clicking failed
HDR-28368 | please add HP 2015 consumer new feature into below PNPID | Ported to trunk. Added HP 2015 consumer new features
HDR-28488 | Gesture and Pointing performance improvement | Set right palm detection flags for hidmini driver.; TL2->TL3.; Only sent one finger up packet for each finger with right confidence. Fixed BSOD when the miniport driver is disabled.
HDR-28584 | PNPID request: 3207 in HPConsumer | Added PNPID SYN3207

Version: 19.0.0 Date: 03-19-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28484 | Create miniport driver INF for major customers. | Created miniport driver installation package for major ciustomers. 1, Added plugin registries back fir miniport driver, otherwise synthenh cannot be launched. 2, Always created OSD class instead of enabling by registry because OSD is used several placec, if this registry is missing, the syntpenh will crash.
HDR-28488 | Gesture and Pointing performance improvement | 1, Fixed memory leakage when the miniport driver is disabled or removed. 2, Fixed the miniport driver is disabled when any USB mouse is unplugged from USB ports. 3, Reported to PTP using normalized X, Y instead of filtered X, Y.; Fixed 1palm+1F failure issue if palm is down first, 1F is down second, then palm is up, the pointing does not work any more. We should fill in finger data one by one from array index 0, should no gap between finger data..
HDR-28545 | Please modify E0 57/E0 58 as lid open/close key | Modified lid open/close key

Version: 18.2.3 Date: 03-12-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28484 | Create miniport driver INF for major customers. | Created miniport driver installation paclage for major ciustomers.

Version: 18.2.2 Date: 03-06-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28341 | Review all INFs to add HID/ACPI before PnP IDs | Per Win10 WU we have to add ACPI before PnP IDS isntead of *.
HDR-28365 | Please modify button height to 1/4 height in Y-axis | Modified the button zone size

Version: 18.2.1 Date: 02-27-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28261 | "EdgeMotion when horizontal scrolling" has no function on touchpad | Configure settings as request.
HDR-28277 | Customer report cursor still can be moved when set power plan to lid do nothing | Add lid close settings to SYN1EFB/1EFC.
PRJ-35549 | Find a solution to enable SMB driver update for specific PnP in WU | Enable SMB driver update for specific PnP in WU

Version: 18.2.0 Date: 02-19-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28225 | PNPID request: SYN3205 for HPConsumer | Added PNPID SYN3205
HDR-28296 | HP request to remove touch injection in below PNPID | Removed touch injection for some PNPIDs
HDR-28297 | PNPID request: SYN3206 for HPConsumer | Added PNPID SYN3206

Version: 18.1.53 Date: 02-12-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28201 | Add below feature into v18.1.7.19_HPConsumer | Modified settings for SYN3200
HDR-28205 | Item ‘"Click -and- Drag" should not list under "Clicking" | Fixed wrong settings; Hide Click and Drag

Version: 18.1.52 Date: 02-05-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28175 | Hide all edge swipe controls for Win10 | Hidden edge swipe controls from CPL for Win10.
HDR-28189 | Add Intel SkyLake chipset support in SMB INF | Added Intel Skylake chipset support for SMBus.
HDR-28085 | Sangriar 2.1/Spritzer 2.1 - Apply HWIDs | Added PNPIDs SYN3203 and SYN3204
HDR-28158 | "Rotating" and "Three-Finger Flick" should be checked in PNPID3202, v18.1.48.51 | Enabled Rotating and Three-Finger Flick

Version: 18.1.51 Date: 01-29-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28038 | [HP/Rocher]Touchpad no function if the system resume from S3 -TM2976 | Fixed Touchpad no function after resume from S3
HDR-747 (1092123) | 1092123 - FNC_PE_HOU/Runt 1.0/Synaptics Touchpad: Touchpad is disabled without external usb device connected with "Disable internal pointing device when external USB pointing device is attached" checked. | Removed extra \ from exclusion list.

Version: 18.1.50 Date: 01-22-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28039 | TouchPad should be enabled after checked "Disable internal pointing device when external USB pointing device is attached" then unplugged external USB mouse. | Fixed the USB mouse plugin/unplugin disable/enable issue, the notification reason is changed, it does not match with user mode driver, so the event is not processed by the user mode driver.,
HDR-23038 (FM: 1256) | Switch to old Control Panel did not see the change made from New Control Panel for four coners in tapzone | Extend timeout to 15 seconds
HDR-28020 | please modify Lid close E0 58, Lid open E0 59 in PNPID 1EFE | Modified lid close/open settings and enabled three finger flick
HDR-28038 | [HP/Rocher]Touchpad no function if the system resume from S3 -TM2976 | Extend timeout to 10 seconds

Version: 18.1.49 Date: 01-15-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-27837 | HP new feature in Consumer UI | Added two finger tapping UI
HDR-27908 | 2015 HP consumer driver setting | Disabled edge swipes for HPConsumer; Removed duplicate section in group
HDR-27989 | branch build request: v18.1.48.x_HPConsumer | Disabled threee finger flick for SYN1EFE

Version: 18.1.48 Date: 01-08-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-27930 | Disable audio feedback for button clicking | Read ForcePad click sound mute status from registry..
HDR-27810 | PNPID request: SYN3202 for HPConsumer | Added PNPID SYN3202
HDR-27837 | HP new feature in Consumer UI | Added two finger tapping UI
HDR-27907 | Please add HWID of Intel new chipset "Braswell" into driver INF | Support Cherryview SMBus Controller.

Version: 18.1.47 Date: 12-25-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Add right button zone adustable UI with certain constraints.
|  | : [ADC] Pls port this code trunk.

Version: 18.1.46 Date: 12-18-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-913 (Hyder001) | Using force data to reduce false taps working with ACM | Ignored tap decoding if force is less than certain threshold.

Version: 18.1.45 Date: 12-11-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-27746 | Add more log information in the driver | Logged ForceModel reset event.
HDR-10234 | HP request TP pinch/zoom performance need to be the same as Touchscreen | Enabled touch injection for pinch to zoom
HDR-10238 | Ubuntu PNPID request: 1EFB 1EFC | [ubuntu] add PNPids for touchpad.
HDR-27721 | HP request when palm is detect, pointing and gesture still should be workable | Enabled gestures when palm is on touchpad
HDR-747 (1092123) | 1092123 - FNC_PE_HOU/Runt 1.0/Synaptics Touchpad: Touchpad is disabled without external usb device connected with "Disable internal pointing device when external USB pointing device is attached" checked. | Added all Synapitcs devices to exclusion list.

Version: 18.1.44 Date: 12-05-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-755 | please add registry to know what scan code we get | Enabled key stroke input log for 1EE8 to 1EEF only
HDR-943 | PNPID request: 1EFF 3200 3201, HPConsumer | Added PNPID 1EFF, 3200 and 3201
HDR-9769 | Please suppress 2f scrolling if 2 finger separate more than 60mm | Enabled 2 finger vertical scrolling horizontal distance threshold

Version: 18.1.43 Date: 11-26-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-832 | please add "scroll to slide" into PNPID 1ED9 and 1EF4 | Enabled scroll to slide

Version: 18.1.42 Date: 11-20-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-363 | "Disable ForcePad Force Progress Bar" has not been translated into Chinese | New translation for Forcepad
HDR-832 | please add "scroll to slide" into PNPID 1ED9 and 1EF4 | Enabled scroll to slide
HDR-837 | HP ubuntu platform: help add scan code for lid close/open | [ubuntu] LID open/close scan code in ubuntu X.
HDR-853 | PNPID request: 1EFE, inf: HPConsumer | Added PNPID 1EFE
HDR-861 | add 1palm 1 finger feature in below PNPID | Enabled one palm and one finger feature

Version: 18.1.41 Date: 11-14-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-747 (1092123) | 1092123 - FNC_PE_HOU/Runt 1.0/Synaptics Touchpad: Touchpad is disabled without external usb device connected with "Disable internal pointing device when external USB pointing device is attached" checked. | Added one PnP ID to exclusion list of mouse.
HDR-754 | please check 1EF5 to 1EF8, to set E0 57, E0 58 as lid open/ lid close | Modified lid close/open key for 1EF5 to 1EF8
HDR-755 | please add registry to know what scan code we get | Enabled key stroke input log
HDR-785 | PNPID request: 1EF9 1EFA, inf: HPConsumer | Added PNPID 1EF9 and 1EFA
HDR-787 | PNPID request: 1EFB 1EFC, HPConsumer | Added PNPID 1EFB and 1EFC
HDR-787 | PNPID request: 1EFB 1EFC, HPConsumer | :[ADC] Pls update PnP list file.
HDR-795 | PNPID request: 1EFD, inf: HPConsumer_RMIHID | Added PNPID 1EFD

Version: 18.1.40 Date: 11-07-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-700 | PNPID request: 1EF4, HPConsumer | Missing AddReg
HDR-700 | PNPID request: 1EF4, HPConsumer | Disabled 3 finger flick and rotating for SYN1EF4
HDR-702 | PNPID request: 1EF5, 1EF6, 1EF7, 1EF8, HPConsumer | Added PNPID 1EF5, 1EF6, 1EF7 and 1EF8

Version: 18.1.39 Date: 10-31-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-626 (ECR232511) | Unqouted Service Path in Registry with SynTPEnhServic | add quotes to Service's ImagePath in Registry
HDR-571 | UI will shift in pike platform, PNPID 1ED9 | Fixed button shifting on Settings property page
HDR-652 | please uncheck "enable edge swipe" and select "static tray icon in taskbar" | Disabled edge swipe and show static tray icon
HDR-672 | please add 97/01 97/02 to notice EC driver get disable/enable scan code | Added notify KBC of 97 command and query KBC for disable State

Version: 18.1.38 Date: 10-24-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-624 | Make DPI aware default disabled | Make DPI aware
HDR-65 | TouchPad doesn't work for a time after detaching external USB mouse | Fixed TouchPad does not work after detaching external mouse
HDR-394 | Win8.1: 0X50 BSOD occur when run WinPMT S3 Focus overnight on WinPMT. | Fixed a BSOD because there was a logic error in checking a pointer is allocated by our MM code or by OS when the pointer was freed, it accidentally added this pointer that is allocated by OS to our free list with wrong size, this caused our MM free list messed up.
HDR-563 | add some edge swipe feature into PNPID 1ED8, 1ED9 | Adjusted edge swipe for 1ED8 and 1ED9
HDR-566 | TouchPad can't be turned off after enabled "Disable" button by HPConsumer.inf. | Rolled back change, it broken TP disable feature if it is TouchPad because the motion is not zeroed out.

Version: 18.1.37 Date: 10-17-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-511 | Pinch does not work in ForceTutorial app | Fixed wrong cursor position when DPI aware is enabled in syntpenh, that caused pinch or scrolling does not work if it uses wheel mouse message and the system is not in 96dpi. Called right function to window handle under pointer to fix wrong window handle which causes pinch does not work in ForcePad Tutorail app.
HDR-499 | Ubuntu platform: PNPID request, 1EAC and 1EDA, traditional TouchPad | [ubuntu] Add PNPids.

Version: 18.1.36 Date: 10-09-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-394 | Win8.1: 0X50 BSOD occur when run WinPMT S3 Focus overnight on WinPMT. | Fixed potential sync. issue in memory management that could cause BSOD.
|  | Modified scan code settings and enable edge swipe for PNPID 1ED9
TP-48741 | [Linux_Ubuntu] Button action selection shouldn't display in Mouse Properties / Settings. | [ubuntu] Remove ClickButtons items on SynTPCpl
TP-48769 | PNPID request: 1EF2 1EF3, HPConsumer | Added PNPID 1EF2 and 1EF3

Version: 18.1.35 Date: 10-02-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28 | [3+2BCP] 3F swipe not working on Metro Photo Application | Make 3F swipe working in Metro Photo Application
HDR-411 | Powerpoint 2013 will be Grayed when using finger to Horizontal scrolling | Used key scroll instead of bar scrolling for PowerPoint to fix "Powerpoint 2013 will be Grayed when using finger to Horizontal scrolling".
HDR-394 | Win8.1: 0X50 BSOD occur when run WinPMT S3 Focus overnight on WinPMT. | Fixed potential memory allocation bug that could cause BSOD.
|  | Removed control zone settings for SYN1ED9, applied the same settings as SYN1ED8
|  | Added PNPID 1EF0 and 1EF1

Version: 18.1.34 Date: 09-25-2014
No changes
Version: 18.1.33 Date: 09-18-2014
No changes
Version: 18.1.32 Date: 09-11-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-264 | Audio feedback missed if clicking is too fast and audio playback is too slow | Queued clicking press/release event, then playback audio feedback one by one if the queue is not empty, this fixed clicking sound missing or press/release misorder.
HDR-136 | The touchpad would lose function for 1 minute after launching the BurnIn | Check BusInterface before using it.
HDR-216 | Scan code modify in below PNPID | Change Lid open/close key and enabledisable key.
HDR-159 | PNPID request: 1EE8, 1EE9, 1EEA, 1EEB, 1EEC, 1EED, 1EEE, 1EEF | Change Lid open/close key and enabledisable key.

Version: 18.1.31 Date: 09-04-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-208 | Remove allowing edge swipe if first three packets are palm | Removed old implementation for relaxing palm rejection in the edge fro edge swipe gestures.
HDR-209 | Add API to disable/enable suppression motion while typing. | Exposed API to allow an application to disable/enable motion suppression while typing.
HDR-210 | Force drag is triggered unexpected | Fix an wrong ForceReleased drag generated by Force-Clciking-releasing without motion before release force.
HDR-227 | Relax edge swipe condition in edge if first three packets are palm | Ignored palm check for first three packets if it is edge swipe, this will fix edge swipe missing with large flat finger or very fast edge swipe.
HDR-136 | The touchpad would lose function for 1 minute after launching the BurnIn | Recovery SMBus Controller by reset it if necessary.
HDR-138 | please unchecked "Double Tap To Enable or Disable TouchPad" in below PNPID | Unchecked "Double Tap To Enable or Disable TouchPad" for PNPID 1EE5, 1EE6 and 1EE7
TP-48497 (1066865) | 1066865 - M-SIT/ BJR_SI2: The OK button will be covered after clicking "Restore All Defaults” button in Synaptics Control Panel. | Adjusted "Restore all Defaults" button size to fix buttons overlap.

Version: 18.1.30 Date: 08-29-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | "Enable" button is not greyed out if the TP is disabled, then plug in USB mouse with "Disable internal pointing device when external USB pointing device is attached" checked.
HDR-108 | Please modify PNPID:1ED9 to HPControl Zone UI | Enabled Control Zone UI for 1ED9
HDR-118 | Please add LID close/open scan code into PNPID:1EA5 | Add "lid open/close" key for HWID SYN1EA5.
HDR-135 | HP confirmed that we need to set "Edge Swipes” to Uncheck as default in PNPID:1ED8 | Uncheked Edge Swipes for PNPID 1ED8
HDR-159 | PNPID request: 1EE8, 1EE9, 1EEA, 1EEB, 1EEC, 1EED, 1EEE, 1EEF | Add new PnPIDs for HPConsumer
HDR-160 | HP request static ICON in system tray in PNPID 1ED8 | Enabled static tray icon for PNPID 1ED8
HDR-173 | HP request right button 30% and left button 70% in PNPID:1ED8 | Adjust button zone size for PNPID 1ED8

Version: 18.1.29 Date: 08-21-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-84 | PNPID request: 1EE5, Avalanche, HPConsumer | Added PNPID 1EE4, 1EE5 and 1EE6
HDR-85 | PNPID request: 1EE6, Glacier, HPConsumer | Added PNPID 1EE4, 1EE5 and 1EE6
HDR-86 | PNPID request: 1EE7, Harvey Flat, HPConsumer | Added PNPID 1EE4, 1EE5 and 1EE6

Version: 18.1.28 Date: 08-15-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-49 | PNPID request: 1EE4, HPConsumer | Added PNPID 1EE4

Version: 18.1.27 Date: 08-07-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48607 | please add E073/ E074 and E057/E058 registry into PNPID:1ED9 | Add lid close/open scan code "E073/E074".

Version: 18.1.26 Date: 08-01-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48491 | PNPID 1EE3, HID/I2C: HP decide to not use control zone feature, please modify driver setting | remove control zone settings of 1EE3.
TP-48494 | PNPID 1ED8 and 1ED9 won't use control zone, please modify the setting to be the same as 1EDC | change default setting to 1EDC's.
TP-48571 | FP-Bullet: Test case 2.5.2 - Resting Palm and Click-and-Drag : FAILED | Fixed one palm + 1F clicking does not work issue on ForcePad.

Version: 18.1.25 Date: 07-25-2014
No changes
Version: 18.1.24 Date: 07-17-2014
No changes
Version: 18.1.23 Date: 07-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47650 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Chinese Simplified | New translations for the word "Charms" for Windows 8
TP-48348 | SynTPEnh crashes when the driver is uninstalled. | Fixed syntpenh crash when the dirver is uninstalled.

Version: 18.1.22 Date: 07-04-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48170 | PNPID request: 1EE0, 1EE1, 1EE2 | Remove the redundant section setting.
TP-48174 | please implement new scan code in below PNPID | Implement new scan code for PNPID SYN1EB1.; Change the setting from HP_GROUP10SGS94UI_RMIHID_Inst to HP_GROUP8SGS94UI_RMIHID_Inst.
TP-48252 | Please add LID close/open scan code into PNPID:1EDD | Add LID close/open scan code into PNPID:1EDD
TP-48289 | Some functions such as horizontal scrolling, vertical scrolling, zoom and rotating can't be checked from Synaptics Luxpad V7.5 after idle about 30 minutes | [Ubuntu] Add PNPid.

Version: 18.1.21 Date: 06-26-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48242 | Remove all short cuts all user when the driver is uninstalled/upgraded. | Remove All users short cuts in uninstallation or before driver update
TP-48174 | please implement new scan code in below PNPID | Implement new scan code

Version: 18.1.20 Date: 06-20-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48028 | 4 finger flick video is wrong in Win7 | Replace 4-finger-flick demo video according to the OS
TP-48094 | Customer cannot call out shortcut menu when tapped touchpad(Synaptics) with two finger | Add functionality of right click when we use 2-finger tap action in Win7. Add default 2FingerTapAction.
TP-48148 | PNPID request: 1EDF, HPConsumer | Add PnPID for HPconsumer.
TP-48170 | PNPID request: 1EE0, 1EE1, 1EE2 | Add PnPID 1EE0, 1EE1, 1EE2

Version: 18.1.19 Date: 06-12-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48028 | 4 finger flick video is wrong in Win7 | Replace 4-finger-flick demo video according to the OS
TP-48095 | It is difficult to move file when one finger pressing left button to choose file and the other finger slide intermittently and fast at the touchpad in the meantime. | changed SuppressPossibleJumps setting.

Version: 18.1.18 Date: 06-06-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48043 | Add TM number in configkey | Appended TM number in configkey so we can support multiple TouchPad in the system.
TP-47988 | Ubuntu platform: PNPID request 1EDB 1EDC | [Ubuntu] FAE wrong information.
TP-47990 | Bottom of Starting Zone was 0%, but according to "20140218_Synaptics_consumer_driver_default...", it should be 15%. | Correct ACM2.0 starting zone path.
TP-48013 | Ubuntu platform: PNPID request 1EAD 1EAE | [Ubuntu] Add PNPids.
TP-48028 | 4 finger flick video is wrong in Win7 | Replace 4-finger-flick demo video

Version: 18.1.17 Date: 05-29-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47921 | please modify "SuppressPossibleJumps" to 0x000000fb in below PNPID | changed SuppressPossibleJumps setting.
TP-47988 | Ubuntu platform: PNPID request 1EBC 1EBD | [Ubuntu] Add PNPid.

Version: 18.1.16 Date: 05-22-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47648 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Brazil Portugese | Fix Portuguese translation for "charms" from Windows 8
TP-47650 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Chinese Simplified | Add translated strings for TouchPad Pointing Speed and 3F Swipe; Fix Traditional and Simplified Chinese words for Win8 Charms
TP-47856 | Text "Momentum" is not translated | Restore translation for "Momentum"
TP-47874 | SynForcePad is not working on SMB or HID/I2C system | Modified the connection type in SynForcePad so we can run the demo app on SMB and other platform.

Version: 18.1.15 Date: 05-15-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47801 | On simplified Chinese language, the translation for "Pointing Speed" is different from the help file on the General tab | Fix Traditional Chinese translation for "Pointer Speed" help topic
TP-47860 | Spell out FW to Firmware | Spelled out FW VErsion to Firmware Version.

Version: 18.1.14 Date: 05-09-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47799 | Set focus on Synaptics device tab | Set focus to Synaptics tab after the CPL is opened.
TP-47814 | Top edge zone size is wrong | Top edge swipe zone size is wrong, whole TP is top edge swipe zone, this causes tue cursor cannot be moved vertically.
TP-47815 | Change FW version display format for HID device | Changed FW version display format for HID device from major.minor to an integer.
TP-47718 | when user move down from top of touchpad, they will see cursor can't move | Fix cursor is frozen when pointing from top/bottom of touchpad.
TP-47744 | PNPID request: 1EDB 1EDC | added pnpids.

Version: 18.1.13 Date: 05-01-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47744 | PNPID request: 1EDB 1EDC | [Ubuntu] Add PNPids.

Version: 18.1.12 Date: 04-25-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47635 | please add PNPID 1EB5, 1EB6, 1EB8, 1EB9 into ubuntu driver | Add PNPid in trunk and modify 1ED5 to touchpad for Ubuntu.
TP-47676 | Unbutu driver: please help remove momentum in UI | Hide momentum option in HP Ubuntu for all clickpad.

Version: 18.1.11 Date: 04-18-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47603 | please do sensor calibration after LID open | 1. Do sensor calibration after LID open 2. Remove enable/disable key.; 1. Do sensor calibration after LID open.
TP-47632 | please modify "SuppressPossibleJumps" to 0x000000fb in below PNPID | changed SuppressPossibleJumps setting for 1EBC, 1EBD.
TP-47633 | PNPID request: 1EDA | Added pnpid.

Version: 18.1.10 Date: 04-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Fixed TP lost function after this power sequence s3->s4->resume.resume from s4, then resume
TP-47381 (1030247) | 1030247 - M-BIOS//Comet/92.50/Win7 64/MV:Put system idle to enter S3 and then S4, touchpad and keyboard lose function after resume. | Fixed TP lost function after this power sequence s3->s4->resume.resume from s4, then resume
TP-47498 | The apps hung up about 10s-25s during closed most recent apps via "Left edge swipe + Inset-swipe + clicking+ down swiped". | Fixed mouse not moving 10-25 seconds after "Left edge swipe + Inset-swipe + clicking+ down swiped".
TP-47534 | Add new video to hpconsumer INF for the TouchPads which have control zone | Videos for all control zone platforms
TP-47550 | please add below PID/VID into inf to prevent TP be disabled by checked "Disable internal pointing device when external USB pointing device is attached" | add pnpids to exclusion list.
TP-47581 | PNPID request: 1ED9, 1ED8 | PnPID request.

Version: 18.1.9 Date: 04-03-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Prevent unnecessary registry reads if stick device is not present.
TP-47221 | Cursor gets stuck inside Application's border | Fixed "Sticky Border" option (in Accessibility options) so that the cursor is not stuck inside application's border after the application is closed.
TP-47287 | TP will be disabled when user checked "Disable internal pointing device when external USB pointing device is attached" | Add more TouchScreen ID into execlusion list.

Version: 18.1.8 Date: 03-27-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47312 | Touchpad drag function insensitive that will drag shorter distance when drag one icon to another place. | Added fix for click-drag delay issue.
TP-47346 | [Linux_Ubuntu] Edge motion should be disabled under default setting | [Linux_Ubuntu] Edge motion should be disabled in default setting.
TP-47438 | please modify PNPID 1ED2 from PS2 to intertouch | changed group name.; changed default settings of 1ED2 back to SMBus.

Version: 18.1.7 Date: 03-21-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46951 | Remove setting remote control region register for AMD SMB driver | Don't touch other bits of ASF_IO index 0x15 register, otherwise ASF does not work after S3/S4/S5.
|  | Added button state in packet when momentum was stopped otherwise drag was dropped after momentum if the button is still down.
|  | Greyed out some controls in main page if the device is disabled.
TP-47287 | TP will be disabled when user checked "Disable internal pointing device when external USB pointing device is attached" | Add TouchScreen ID into execlusion list.

Version: 18.1.6 Date: 03-13-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Show disable TP when mouse connected checkbox in settings dialog
TP-47125 (1014770) | 1014770 - Cannot resume to OS from S3/S4/S5. | The machine cannot be resumed to OS from S3/S4/S5 by ASF command because the driver disabled ASF..
TP-47136 | HP define LID close/open scan code, and will use in all systemand all ODM in the future | Changed lid close/open scan code.
TP-47278 | please change to PS2 in PNPID 1EBC and 1EBD | Changed default setting of 1EBC, 1EBD, 1ED2 to PS2.
TP-47313 | PNPID request: 1ED6, 1ED7 | Added PNPID 1ED6, 1ED7.
TP-47317 | please change PNPID 1ED2 to PS2 interface | changed default settings of 1ED2 to PS2.

Version: 18.1.5 Date: 03-06-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47150 | [HP Control zone] Top edge swipe is trigged in desktop, and it will cause cursor can't move | Also set booleans false.
TP-47207 | All opened apps will close when doing Left wing Click + Inset-swipe + down swipe | Fixed all opened apps will close when doing Left wing Click + Inset-swipe + down swipe.
TP-47249 | Ubuntu platform: please add PNPID into ubuntu driver | Add PNPID to Linux Build for HPConsumer
TP-47261 | PNPID request: 1ED5 | Add pnpid
TP-47278 | please change to PS2 in PNPID 1EBC and 1EBD | changed default settings of 1EBC, 1EBD to PS2

Version: 18.1.4 Date: 02-27-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47170 | customer report filter activation time is in 0/6, correct setting should be in 2/6 | Modified PalmCheck filters registry path to get settings for either ACM1 or ACM2.0.; Set advanced filter timeout to notch 2 (1sec).
TP-46803 | please checked "2 finger scrolling=>Enable Coasting", then the slide setting is 9/11 | Set 2 finger scrolling coasting slider to 9/11 in default.
TP-46923 | Quanta report TP sometime lose function after boot, and TP will recover after boot again | New SMBus controller support for AMD Beema.

Version: 18.1.3 Date: 02-21-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46489 | "Synaptics TouchPad" will become "HP Control Zone" after dash image | Removed “HPControlZone.lnk” in all platforms.
TP-46803 | please checked "2 finger scrolling=>Enable Coasting", then the slide setting is 9/11 | Added settings to check "2 finger scrolling Enable Coasting", set slider to 9/11.
TP-47136 | HP define LID close/open scan code, and will use in all systemand all ODM in the future | Added lid close/open scan code.
TP-47147 | please change PNPID 1ED3 to group114 | Changed 1ED3 to HP Control Zone platform setting.
TP-47150 | [HP Control zone] Top edge swipe is trigged in desktop, and it will cause cursor can't move | Fixed Top edge swipe is trigged in desktop, and it will cause cursor can't move.

Version: 18.1.2 Date: 02-13-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45105 | difficult to move touchpad at the first time after open lid | Support re-calibration in RMI mode.
TP-47004 | The function of edge swipes is still available while disabled Edge Swipes in "HP Control Zone" UI. | Fix Edge Swipe Enable control when both wingzone and edge swipe zone co-exist

Version: 18.1.1 Date: 02-07-2014
No changes
Version: 18.1.0 Date: 01-30-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46951 | Remove setting remote control region register for AMD SMB driver | Removed unnecessary code to change the slave address of AMD SMB controller1 for ASF, this caused NIC fails to talk with SMB ASF.
TP-46887 | please change 1EB1 to SMBus driver | Changed 1EB1 to SMBus.

Version: 18.0.9 Date: 01-23-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46620 | Localize ForcePad User Guide HTML | Fix Arabic phrases and language selection bar; New translations for HP Quickstart Guide.; Merge Indonesian language translation for Quickstart Guide
TP-46887 | please change 1EB1 to SMBus driver | Changed 1EB1 to SMBus.

Version: 18.0.8 Date: 01-16-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46620 | Localize ForcePad User Guide HTML | Add new language files (still untranslated) to HP Quickstart Guide; Add new languages for HP HTML guide; Update build scripts and HTML files; Add a few more languages to HP user guide HTML project; Fix more language issues in HTML files; Localize ForcePad User Guide HTML.
TP-46752 | please modify the button area to 30%right and 70%left in Group100 | [ADC] Do you also need to adjust LeftButtonR to 67%?
TP-46803 | please checked "2 finger scrolling=>Enable Coasting", then the slide setting is 9/11 | Added settings to check "2 finger scrolling Enable Coasting", set slider to 9/11.
TP-46818 | please checked "Double Tap to Enable or Disable TouchPad" in PNPID 1EC4 and 1EAC | Checked "Double Tap to Enable or Disable TouchPad" for 1EC4 and 1EAC.

Version: 18.0.7 Date: 01-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46476 | [ACM2.0] Edge swipes | Eliminated accidental edge swipe while a finger moved to edge area of TouchPad.
TP-46588 | New Video for SGS94 and UX_UI | Updated Control Panel Help Video files.
TP-46749 | Improve 2F scrolling and inertial by using history data | Remove flag that is no longer used. Improve scrolling and inertia by using history data. Update 2FScrolling inertia settings for improved 2F scrolling. Change Inertia speed to be consistent with current settings.
TP-46625 | "Synaptics Pointing Device Driver" shown in program and feature, this setting is different as Rango's setting | Fixed issue of "Synaptics Pointing Device Driver" shown in Programs and Features on control zone platforms when using System Recovery.
TP-46626 | TM2960-001 Top edge swipe is trigged in desktop, and it will cause cursor can't move | Fixed Top edge swipe trigged in Windows desktop, and it will cause cursor not moving.
TP-46677 | PNPID request: 1ED4 | Change SYN1ED4 setting to same as SYN1ECA.
TP-46680 | HP Fiona: Cursor will move when clicking clickpad | Fixed cursor jumping when one finger clicking
TP-46713 | please help modify setting of below PNPID | Changed to 1ED4's setting.
TP-46743 | please modify the button area to 50%right and 50%left in Group100 | Set left and right button zone size equal.
TP-46752 | please modify the button area to 30%right and 70%left in Group100 | Changed button zone size back to 30% right and 70% left.

Version: 18.0.6 Date: 12-27-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46677 | PNPID request: 1ED4 | Add PNPid 1ED4 for HPConsumer.

Version: 18.0.5 Date: 12-20-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46624 | Suppress Palm Clicking for ForcePad | Suppressed palm clicking for ForcePad.
TP-46574 | PNPID request: 1ECB 1ECC 1ECD 1ECE 1ECF 1ED0 1ED1 1ED2 1ED3 | Added PNPIds.
TP-46586 | Traditional Edge Swipes can't be Checked in the seetings from HP Control Zone properties | Fixed Traditional Edge Swipes GUI not working in Control Zone properties.

Version: 18.0.4 Date: 12-12-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46538 | HP Phelps: cursor moving will delay for a while when "1 finger in button zone" | Fixed cursor moving will delay for a while when a finger is in button zone.
TP-46548 | HP Ubuntu platform: Synaptics driver install error: | For traditional linux PS2 TP driver, we still need to claim PNP0F13.

Version: 18.0.3 Date: 12-06-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Lower the warning level to avoid annoying debug message.
TP-46526 | Unexpected Click when a finger moves out of TouchPad from edge | Fixed unexpected click when a finger moves out of the ForcePad from edge.
TP-46379 | Ubuntu driver request | PnPID request for PS/2 device on Ubuntu.

Version: 18.0.2 Date: 11-27-2013
No changes
Version: 18.0.1 Date: 11-21-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46244 | Clicking is suppressed in some conditions | Fixed WingZone Clicking is suppressed in some conditions.
TP-46368 | PNPID request: 1EC5, 1EC6, 1EC7 | Added PNPIDs.
TP-46401 | PNPID request: 1EC9 1ECA | Added PNPIDs.

Version: 18.0.0 Date: 11-14-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46243 | Difference performance of 2 Finger Tap | Wait 20ms delay and retry ModeSwitch until it is sucessful or timeout.
TP-45429 | HP Rango : Cursor will be moved when we use Top Edge Swipe to trigger an action. | Fixed Cursor moving issue when we use Top Edge Swipe to trigger an action.
TP-46244 | Clicking is suppressed in some conditions | Fixed WingZone Clicking is suppressed in some conditions.
TP-46256 | PNPID request: 1EBC 1EBD 1EBE 1EBF 1EC0 1EC1 1EC2 1EC3 | Added PNPIds.
TP-46287 | please provide registry to modify setting and modify setting into trunk build | Unchecked 'Double Tap to Enable or Disable TouchPad'.
TP-46293 | The "HP control zone Disable” will be cut off as below screen shot | Fixed "Control Zone Disable" string cut off issue.; Fixed "Control Zone Disable" string cut off issue.
TP-46312 | please add scan code to disable/enable TP | Add disable/enable TP via scan code feature.

Version: 17.1.1 Date: 11-07-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46162 | HP-_project_: Unable to set EdgeMotion Speed faster than default | Increased maximum edgemotion speed which has more selections from the edge motion speed slider.
TP-46206 | Locking Drag has no function in OEM INF | Fixed Lock Drag no funtion issuel.
TP-46218 | Calculate the force after TPFiler | Calculate the force after TPFiler
TP-46220 | Make ClickDrag edgemotion on ForcePad | Made ClickDrag edgemotion work after force calculation was moved after CTPFilter.
TP-46046 | Touchpad left shortcut gesture no function after resuming from via open lid. | FollowUp:Remove commented out code and correct NeeCheck to NeedCheck.
TP-46212 | PNPID request: 1EB8 1EB9 | Added pnpids.
TP-46223 | HP Rango : Two fingers tap needs to report right button action on Win7 OS | Enabled Two Finger Tap to report right button action on Windows 7.

Version: 17.1.0 Date: 10-31-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45899 | Add Code for supporting Legacy TouchPad PC settings opt-in on win 8.1 | Add code to support Legacy touchpad setting on win8.1
TP-45967 | BSOD on version 17.0.8.11 | Check IRQL before calling KeClearEvent.
TP-46066 | 2F click & drag terminates when the force is relaxed = make it similar to 1F click & drag | Added code to support 2F drag with force released.
TP-46082 | BSOD after S3 resume | Move startTimer in front of syn function.
TP-46046 | Touchpad left shortcut gesture no function after resuming from via open lid. | Add ConfigFlags to ignore checking system lid close event.
TP-46131 | The system will pop up "64-bit Touchpad control panel extensions has stopped working” | Fixed control panel crash when applied UI changes. It only happed if you launch Synaptic Touchpad V7.5 on system control panel.

Version: 17.0.20 Date: 10-25-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46014 | OEMWPF and OEMWPF_RMIHID: TP can't work after drag file with DragLock function enabled with TP v17.0.17.0 | Added fix to release drag lock after 500ms timeout, and not make touchpad frozen. Update code to allow dribble packets to be sent, but not mess other sending group packets.
TP-46092 | please change 1EB1 to PS2 mode | Changed 1EB1 to PS2.
TP-46096 | PNPID request: 1EB6 | Added pnpid

Version: 17.0.19 Date: 10-17-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45281 | Click action is not consistent | Fixed the issue which checked wrong registry control for enabling/disabling 1Palm+MF clicking.
TP-45755 | resting palm + 1F click or 2F click support | Removed TL2s.
TP-45976 | Skip force calculation for Palm | Skipped force calculation if there is only palm without any finger.
TP-45999 | PNPID request: 1EB4, 1EB5 | Added PNPIDs.

Version: 17.0.18 Date: 10-11-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45934 | Add different force release threshold for 2F drag there is one finger in the button | Added another force release threshold for 1F resting + another finger drag.
TP-45976 | Skip force calculation for Palm | Skipped force calculation for palm object.; Skipped force calculation if there is only palm without any finger.
TP-45977 | Add "Enable Force" in the tray icon to disable/enable force continuation. | Added control option "Enable Force" in tray icon that allows end user to enable/disable force conitnuation pinch and scrolling, and 2F clicking.
TP-44027 | Add UI to switch tranditional edge swipe and HP advanced edge swipe | [ADC] Can we remove the code that did this the old way?
TP-45472 | 2F scrolling + resting finger is noticably slower/jerkier than without resting finger | Fixed Two Finger scrolling + inertia not working issue.
TP-45927 | HP Rango - Please add workaround to reduce driver detection timing when system from S3 to S4 | Add ReadDeviceInfoFromRegistry mechanism.; Only ignore MultiPhy capability with IOCTL case.
TP-45939 | PNPID request: 1EB0, 1EB1, 1EB2, 1EB3 | Added PNPIDs. Modified 1EB1's settings.

Version: 17.0.17 Date: 10-03-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45281 | Click action is not consistent | Added registry control to enable/disable 1Palm+MF clicking.
TP-45755 | resting palm + 1F click or 2F click support | 1, Used ClickSmart for 2F click in ForcePad, we don't need to consider the force. 2, Made 1Palm+1F and 2F click work.
TP-45756 | resting palm + 2F tap | Fixed bit mask. Reimplemented MF tap with resting fingers in button zone.
TP-45918 | Add FW RawPacket Position filter to the driver | Add FW RawPacket Position filter to the driver
TP-45674 | The Smart Sense-Starting zone show "Bottom: 10%", please modify to "Bottom: 15%" | Changed starting zone size settings.
TP-45777 | Remove Synaptics brand name from uninstallation page | Removed Synaptics brand name from uninstallation page.; [ADC] Change the unit in the reg name to either Um or Microns.
TP-45812 | Merged HP Rango feature into main trunk | Merged HP Rango branch into main trunk. Merged HP Rango branch into main trunk.
TP-45873 | default setting modify: PNPID:1EAC | Uncheck "Double Tap to Enable or Disable TouchPad".
TP-45892 | PNPID request: 1EAF | Added PNPID
TP-45917 | Adjust left wing zone size for PS2 mode | Adjusted left wing gesture zone size for PS2 mode.

Version: 17.0.16 Date: 09-26-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44750 (20130628 meeting with Kirk) | After log file capture Kirk would like the default folder opened so that the log file can be copied or viewed instead of just closing | Add option for user to open log file folder after collecting diagnostic info
TP-45827 | Add option to show progress either in current command prompt window or show it in another command prompt window title | Added an option to show progress either in current command prompt window or show it in another command prompt window title
TP-44027 | Add UI to switch tranditional edge swipe and HP advanced edge swipe | make the wing pull ioctls be a eeiDisableGestures bit.
TP-45777 | Remove Synaptics brand name from uninstallation page | Removed Synaptics brand name from uninstallation page.
TP-45812 | Merged HP Rango feature into main trunk | Merged HP Rango branch into main trunk. fix a merge error for ForcePad.
TP-45832 | please modify PNPID 1EAD, 1EAE from group106 to group95 | Modify setting from InterTouch to PS/2.

Version: 17.0.15 Date: 09-19-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Added HID mouse filter callback functions.
TP-45582 | BSoD on WHCK test | Keyboard filter driver should pass specific IOCTL to function driver.
TP-45786 | BSOD 0x1E occur when customer uninstall driver | For uninstall case, we still need to unregister notification handler.
TP-45792 | 988033 Touchpad cannot be disabled/Enabled by hotkey(Fn+f2)on bullet unit | Fix Mux KBC if touchpad is connected to port 1, 2 or 3.
TP-45801 | Keep motion/tap/gesture suppression after palm before timeout | Last palm time stamp variables were reset. Fix "keep motion/tap/gesture suppressed after palm before timeout" feature.
TP-45803 | Show right asic type from Diag. page | Show right ASIC type for 1320 and 1321 on Diag. page.
TP-45105 | difficult to move touchpad at the first time after open lid | The BIOS of that platform has capability to notify driver about lid close/open status. Caused FW need be re-calibrated during some specific timing, EC will use lid close/open scan code for this purpose. Turn off the notification on this platform.
TP-45497 | customer report right button area is too small, please adjust to left:right =6:4 | Corrected comment.
TP-45745 | Why LCD will be on when system wake up from S3 via WOL with AMD Kabini platform? | Disable KBC 0x97 command notify
TP-45784 | please disable TP when get lid/close scan code | Added lid open/close scan code.

Version: 17.0.14 Date: 09-13-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45582 | BSoD on WHCK test | Fix BSOD when doing system WHCK test
TP-45663 | BSOD for WHCK "Fault Injection Test" | Fix WHCK Fault Injection Test
TP-45496 | Edge swipes gesture is easily trigger when move the finger on the Clickpad (About 1cm area move finger at the edge of the TP) | Changed edge swipe zone setting.
TP-45594 | when customer open our UI, there is additional rectangle pop up | Fixed issue of an abnormal grey rectangle showing up when launching our UI from "Synaptics ClickPad V..." in control panel.
TP-45703 | When click clickpad and without finger position, driver will recognize as left button function. Customer want driver just do nothing | Added setting to disable "force left click when no finger".

Version: 17.0.13 Date: 09-05-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44637 | Testarossa - BITS087995: [PT_TSA]Sometimes mouse cursor don't change icon as scrolling | Added fix to show custom cursor correctly.
TP-45194 | English description on Simplified Chinese OS | Update translations
TP-45590 | BSOD 0x10D occur when doing Restart,S3 and S4 +LAN (Right usb port) 14 hours | Unregister RMI callback func before register it.
TP-45260 | Add HP branding name for HP Rango | [ADC] m_UserStaticBmp->m_oemStaticBmp.
TP-45505 | Can't enable touchpad by double click upper-left of touchpad if enable this function from touchpad settings without click "apply" then close | Do not close CPL when device is disabled.
TP-45593 | please help modify "Synaptics PS/2 TouchPad" to "Synaptics PS/2 ClickPad" in Device Manager | Changed device description in device manager.
TP-45621 | Edge swipes gesture is easily trigger when move the finger on the Clickpad (About 1cm area move finger at the edge of the TP) | Adjust Edge Swipe Zone.

Version: 17.0.12 Date: 08-30-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45504 | Spyder ULT - There is no function after install driver | Pass the WdfRequest handle to the WDF function .
TP-45105 | difficult to move touchpad at the first time after open lid | Set lid open action to re-calibrate, it could help FW for noise issue. After Re-Calibration, driver should also enable device.
TP-45340 | PNPID request: 1EAC , in v17.0.8_HPConsumer and above. | Added PNPID 1EAC to trunk.
TP-45495 | PNPID request: 1EAD, 1EAE, inf:HPConsumer | Added PNPIDs.
TP-45496 | Edge swipes gesture is easily trigger when move the finger on the Clickpad (About 1cm area move finger at the edge of the TP) | Changed edge swipe zone setting.
TP-45497 | customer report right button area is too small, please adjust to left:right =6:4 | Adjusted button zone size.

Version: 17.0.11 Date: 08-23-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45258 | OEM_project_ (SYN1E62) - BSOD after installing v17.0.9 driver | Use InterlockedExchange() and add comments.
TP-44027 | Add UI to switch tranditional edge swipe and HP advanced edge swipe | [ADC] Double check with Niahm if these are the strings that HP wants.
TP-45260 | Add HP branding name for HP Rango | Add HP branding name for HP Rango.
TP-45340 | PNPID request: 1EAC , in v17.0.8_HPConsumer and above. | Added new PNPID.
TP-45401 | Opening TP UI, it should show SmartSense not show PalmCheck-Enhanced. please change the name | Modified palm check caption.

Version: 17.0.10 Date: 08-15-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45096 | Device fails detection after reflashing fw using SynapticsReflash found in v17_0_7 | Fixed Device fails detection after reflashing fw
TP-45258 | OEM_project_ (SYN1E62) - BSOD after installing v17.0.9 driver | Use atomic variable to avoid reentry and add timeout mechanism as well.
TP-45272 | Please gray out the "Filter Activation Time", when uncheck "Restrict pointing to zone" and "Restrict tapping to zone" | Gray out "Filter Activation Time", when uncheck "Restrict pointing to zone" and "Restrict tapping to zone".

Version: 17.0.9.1 Date: 08-14-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45258 | OEMEnvy (SYN1E62) - BSOD after installing v17.0.9 driver | Rollback codes. It seems problem to call Mutex acquire function in DPC.

Version: 17.0.9 Date: 08-08-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45025 | After use touchpad to reboot system, it would BSOD in OS | Check IRQL before calling RtlQueryRegistryValues function.
TP-45111 | Mode switch failed on Win8.1 | Suppor OEM SMBus Host Controller.
TP-45147 | Cusor jumps with OEM 5BFP | Add mechanism to avoid reentry for SMBus driver. Port reentry avoidance mechanism to CRMIPort.

Version: 17.0.8 Date: 08-01-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-42303 | Improve Driver build process and release note for customers | Remove useless notification in middle of build; Fix file verification script; Fix UTF-8 failure to translate non-ASCII apostrophe in release notes
TP-44354 | Horizontal two finger scrolling can't work on PDF file via win8 PFD APP | Fix horizontal scrolling becomes vertical scrolling in Metro simple Chinese pdf reader
TP-44770 | Bonsai - Can not use zoom in/out function after put a third or more fingers on the touchpad | Avoid canceling pinch action when more finger down feature is set.
TP-44975 | WHCK Failure (PS/2) - 17.0.5.3 | HPConsumer.inf (Next/Blue) | Added Synaptics generic compatible ID *SYN0002 for all PS2 touchpad infs; Added a hack until Microsoft fixes its WHCK tool
TP-45042 | Scrolling is not smoothly on metro app Photos and Camera while ZoomPerfect is enabled | Fix injection error for 2 finger scrolling gesture under Metro-mode app. This error will cause scrolling not smooth.
TP-44026 | Implement new left edge and right swipe per HP request | Implement new left edge and right edge gestures on Windows 8.
TP-44993 | [Win7 64bit] System will pop up "Stopped working" msg during re-install Touchpad driver by Recovery Manager (PNPID= 1EA6) | Fixed memory access violation that results in "Stopped working" pop-up msg during re-install driver by Recovery Manager.

Version: 17.0.7 Date: 07-26-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44571 | Spyder ULT - Default setting is incorrect | Duplicate of ClickpadViews, ClickpadViewModel for OEM Win7 UI for 2013.
TP-44879 | OEMWPF TPPB - modified Win7 UI for 2013 | Changed help text. Added new help text, all in English for now.
TP-44999 | Edge motion does not work | Enable EdgeMotion feature by default for Rango.
TP-45005 | Adjust cursor speed | Increase pointing speed
TP-45040 | please add the fix of TP-44967 into trunk | Added settings to disable/enable device by lid close/open.

Version: 17.0.6 Date: 07-18-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Display ACM 2.0 type in Diagnostic panel
TP-44941 | Getting wrong register offset of ACM20 existence for old FW | Parsing ACM2.0 existence information correctly.; Update the packrat number.; Provide ACM2.0 disabled setting.
TP-44863 | HP Rango : Modify Smart Sense setting by default, PNPID = SYN1EA7 | Added settings of advanced filters for Rango.

Version: 17.0.5 Date: 07-11-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Follow-up: add registry overrides for RMI4 caps; Add RMI4 capabilities query to API
TP-44188 | Customer wants previous release notes combined with current release notes | Add a "history" feature to ReleaseNotes.HTML; Build script now creates a history from previous release notes
TP-44828 (958966) | It will pop up the error "SynTPEnh.exe-Entry Point Not Found" at the end of insttalling Synaptics driver on Vista 32&64. | Fixed SynTPEnh and SynTPHelper crash in Vista with driver built with Vs2012
TP-44027 | Add UI to switch tranditional edge swipe and HP advanced edge swipe | Add UI to switch tranditional edge swipe and advanced edge swipe
TP-44789 | Please remove the date in Synaptics UI | Added setting to not show driver version date on UI. Moved setting to HP common setting.
TP-44865 | please enlarge the top swipe area | Changed top edge swipe setting for SYN1EA3, SYN1EA4

Version: 17.0.4 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Do fixme and handle F11 data offsets properly. Still a wip since a large number of F11 data registers remain unchecked in the interrupt handler.
TP-44721 | Geasture issue on Google Chromewith High DPI setting | Fixed issue of two finger scrolling not working when cursor is near the right edge of the window with DPI=150%
TP-44750 (20130628 meeting with Kirk) | After log file capture Kirk would like the default folder opened so that the log file can be copied or viewed instead of just closing | In Windows 8.1 Preview, the GetVersion(Ex) APIs have been deprecated.; In Windows 8.1 Preview, the GetVersion(Ex) APIs have been deprecated. Update Manifest
TP-44026 | Implement new left edge and right swipe per HP request | Implement new left edge and right edge gestures on Windows 8.
TP-44738 | please enlarge the top swipe area | Changed edge swipe settings for SYN1EA5
TP-44756 | System WHCK test item “Touch Tool” fail with 17.0.2.2 | Fixed System WHCK test item Touch Tool failures.

Version: 17.0.3 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-42303 | Improve Driver build process and release note for customers | For release notes, if "Contact" field is missing, print the Creator of the Jira issue; Create a default empty dictionary in case JSON load fails for invalid and missing Jira numbers; Use Python decode('utf-8-sig') to strip byte order mark out of text; Do not distribute Release.txt any more since it is not updated. Use ReleaseNotes.html.
TP-43964 | ACM 2.0 change of algorithm strength driver meta-bug | Make contact type interface consistent. Add HasACM2() query.
TP-44618 (TM-2768-001) | The systray icons will flicker when scrolling in a photos viewer with three finger flick | Only turned on IME workaround for twist action instead of all gestures for Photo Viewer.
TP-44682 | Use maximum force instead of total force for multiple fingers click | Used maximum force instead of total force for MF click.
TP-44692 (ECR177029, ECR176429) | Copyright issue | Update Coypyright to 1996-2013
TP-44026 | Implement new left edge and right swipe per HP request | Implement new left edge and right edge gestures on Windows 8.; Follow Up [ADC] Rename "app bar width" to "activaiton threshold"; Refactor the check for finger counts in the idle state.
TP-44263 | HP Rango Platforms PnP ID | Added Rango Platforms PnP ID
TP-44680 | Please change the setting of PNPID:1EAB | Changed settings for SYN1EAB

Version: 17.0.2 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44299 | Right side, down side "Return at edge of screen" in Momentum doesn't work | Fixed the bounce off screen edge in momentum not working issue with high DPI.
TP-44026 | Implement new left edge and right swipe per HP request | Implement new left edge and right edge gestures on Windows 8.
TP-44562 | [Linux] Empty main window "property of Synaptics LuxPad V7.5" | Fix an issue that device list in Linux control panel is empty

Version: 17.0.1 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44440 | Convert packet count to time | Improve taps-Convert packet count to time.; Make gesture work properly for different report rates of devices; Make PalmOnPad gesture works normal for various report rate of devices.; code improve by rename a function.; Add a utility function to clear packet.
TP-44531 | Silent Uninstallation fail in in toshiba.inf | Silent Uninstallation fail with SynIsdll built with Vs2012; Silent Uninstallation fail in in Win8 x64
TP-44533 | Application crashes when we double tap on the top left corner of the TP to disable the touchpad in HPNEWUI v17.0.0 | Changed call convention from std to cdecl to fix syntpenh creash when it reads Png file.
TP-44564 | ACM2.0 can't work on OEM machine | FollowUp:Change uiQuery36Offset -- to uiQuery36Offset--.; Correct RMI query parsing.
TP-44026 | Implement new left edge and right swipe per HP request | Implement new left edge and right edge gestures on Windows 8.; Implement new left edge and right edge gestures on Windows 8.
TP-44552 | PNPID request: 1EAB | Added new PnPID

Version: 17.0.0 Date: 06-07-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44045 | _project_ (175) - Tap to click will invalid for few seconds after 2 or 3 finger slide on pad | Improve conmunication between API and Kernel Driver.;
TP-44046 | _project_ (176) - Continue tap the 2-finger on the touchpad surface will always trigger both of mouse right and left button events. | Improve tap vs drag with 1F and multifingers, as well as communication between API and Kernel Driver..
TP-44244 | Task tray Synaptics icon, "Pressure graph" and "MoodPad" items cannot be seen. | Fixed the wrong location of popmenu by right clicking trayicon, when the size of all items is set to 150% in control panel.
TP-44299 | Right side, down side "Return at edge of screen" in Momentum doesn't work | Fixed the bounce off screen edge in momentum not working issue, when the size of all items is set to 150% in control panel.
TP-44300 | Enable Tap zone, even touch right up corner, Maximum windows doesn't work | Fixed the issue of maximizing windows not working, when the size of all items is set to 150% in control panel.
TP-44348 | Switch from VS2005 to VS2012 by Default | Save 2005 solution; Switch from VS2005 to VS2012 by Default Use include and lib files from T drive; Bump SynTPCo19.dll to SynTPCo20.dll; SynDell;share\Png; Solution files; KmdfLibraryVersion = 1.11, WdfCoInstaller01011.dll; SynOsLib dir.lst; Remove ...2012.sln files; Inf2Cat; forcetext2bin; Use Include and lib files from T drive
TP-44457 | 16.6.5 sony2006.inf Two-Finger horizontal scroll failed. | Only read application specific settings when apps switch happens, otherwise some user specific settings will be overridden if CPL is opened and changes are not apllied.
TP-44026 | Implement new left edge and right swipe per HP request | Follow Up [ADC] Instead of using packet counts, use the time deltas. Try turning on the "cursor highlight with control key" option, and check if this causes a problem.; Implement new left edge and right edge gestures on Windows 8.; Implement new left edge and right edge gestures on Windows 8.
TP-44263 | HP Rango Platforms PnP ID | Added Rango Platforms PnP ID
|  | Restored 1EA4 and 1EA5 settings.