;=====================================================
;
;   G246HYL.inf         Ver. 1.0      02/19/2013
;
;   Copyright (C) 1999-2009 Acer Inc.
;
;   This is a Microsoft Windows setup information
;   file for the Acer Color Monitor.
;
;=====================================================
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%Acer%
DriverVer=02/19/2013, 1.0.0.0

; Ensure to add directive below with the proper catalog file after WHQL
; certification
CatalogFile=G246HYL.cat

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
DefaultDestDir=11
G246HYL_Analog.copyfiles = 23
G246HYL_Digital.copyfiles = 23
G246HYL_HDMI.copyfiles = 23

[SourceDisksNames]
1=%SourceDisksNames%

; Enable the following section to copy a monitor profile
[SourceDisksFiles]
G246HYL.icm=1

[Manufacturer]
%Acer%=Acer,NTx86,NTamd64

[Acer]
%G246HYL_Analog%=G246HYL_Analog.Install, MONITOR\ACR035B
%G246HYL_Digital%=G246HYL_Digital.Install, MONITOR\ACR035B
%G246HYL_HDMI%=G246HYL_HDMI.Install, MONITOR\ACR035B

; Modify the hardware ID (ACR035B) to match that of the monitor being used
[Acer.NTx86]
%G246HYL_Analog%=G246HYL_Analog.Install, MONITOR\ACR035B
%G246HYL_Digital%=G246HYL_Digital.Install, MONITOR\ACR035B
%G246HYL_HDMI%=G246HYL_HDMI.Install, MONITOR\ACR035B

; Modify the hardware ID (ACR035B) to match that of the monitor being used
[Acer.NTAMD64]
%G246HYL_Analog%=G246HYL_Analog.Install, MONITOR\ACR035B
%G246HYL_Digital%=G246HYL_Digital.Install, MONITOR\ACR035B
%G246HYL_HDMI%=G246HYL_HDMI.Install, MONITOR\ACR035B

[ControlFlags]
ExcludeFromSelect.NT=Monitor\ACR035B
ExcludeFromSelect.NT=Monitor\ACR035B

[G246HYL_Analog.Install]
ACRReg=ACR_CURRENT_REG
AddReg=G246HYL_Analog.AddReg, 1920, DPMS
CopyFiles=G246HYL_Analog.CopyFiles

[G246HYL_Digital.Install]
ACRReg=ACR_CURRENT_REG
AddReg=G246HYL_Digital.AddReg, 1920, DPMS
CopyFiles=G246HYL_Digital.CopyFiles

[G246HYL_HDMI.Install]
ACRReg=ACR_CURRENT_REG
AddReg=G246HYL_HDMI.AddReg, 1920, DPMS
CopyFiles=G246HYL_HDMI.CopyFiles


[ACR_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

; Pre-defined AddReg sections. These can be used for default settings on
; a given standard resolution is used.

[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[G246HYL_Analog.AddReg]
HKR,"MODES\1920,1080",Mode1,,"31.0-75.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"G246HYL.icm"

; Enable the following section to copy a monitor profile
[G246HYL_Analog.CopyFiles]
G246HYL.ICM

[G246HYL_Digital.AddReg]
HKR,"MODES\1920,1080",Mode1,,"31.0-75.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"G246HYL.icm"

; Enable the following section to copy a monitor profile
[G246HYL_Digital.CopyFiles]
G246HYL.ICM

[G246HYL_HDMI.AddReg]
HKR,"MODES\1920,1080",Mode1,,"31.0-75.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"G246HYL.icm"

; Enable the following section to copy a monitor profile
[G246HYL_HDMI.CopyFiles]
G246HYL.ICM

[Strings]
MonitorClassName="Monitor"
Acer="Acer Inc."
SourceDisksNames="Acer Inc. Monitor G246HYL Installation Disk"

G246HYL_Analog="G246HYL(Analog)"
G246HYL_Digital="G246HYL(Digital)"
G246HYL_HDMI="G246HYL(HDMI)"


